

**MODEL: TX880 SPK**

PICTURE



**SPECIFICATION**

|  |  |
| --- | --- |
| Type | Transducer Moving coil dynamic speaker |
| Impedance | 90Ω±15% @1KHZ |
| Sensitivity | 120±3dB @1KHZ |
| Resonance freq | (F0) 400HZ±20% |
| Frequency respond | F0~9KHz |
| Rated input power | 500mW |
| Maximum input power | 1000mW |
| Suitable for | Earphone TX880,TX885,TX850,TX880L series |