**MODEL: TX880 SPK**

PICTURE

**SPECIFICATION**

|  |  |
| --- | --- |
| Type |  Transducer Moving coil dynamic speaker |
| Impedance |  90Ω±15% @1KHZ |
| Sensitivity |  120±3dB @1KHZ |
| Resonance freq |  (F0) 400HZ±20% |
| Frequency respond |  F0~9KHz |
| Rated input power |  500mW |
| Maximum input power |  1000mW |
| Suitable for | Earphone TX880,TX885,TX850,TX880L series |